Jump to main content

##

# 2.120.2.41 TC_COMPARE_STATUS Enum

## C

    typedef enum
    {
        TC_COMPARE_NONE  = 0U,
        TC_COMPARE_A = TC_SR_CPAS_Msk,
        TC_COMPARE_B = TC_SR_CPBS_Msk,
        TC_COMPARE_C = TC_SR_CPCS_Msk,
        TC_COMPARE_STATUS_MSK = TC_SR_CPAS_Msk | TC_SR_CPBS_Msk | TC_SR_CPCS_Msk,
    }TC_COMPARE_STATUS;

## Summary

Identifies channel interrupt source mask

## Description

This enumeration identifies TC compare mode interrupt source mask.

## Remarks

None.