Jump to main content

##

# 2.120.2.15 TCx_CHy_CompareStart Function

## C

    /* x = TC instance number, y = channel number */
    void TCx_CHy_CompareStart ( void )

## Summary

Starts the given TC channel compare counter.

## Description

This function enables the clock and starts the counter of associated channel in compare mode so that the TC module may start generating the selected waveform.

## Precondition

TCx_CHy_CompareInitialize() function must have been called first for the given channel.

## Parameters

None

## Returns

None.

## Example

    TC0_CH1_CompareInitialize();
    TC0_CH1_CompareStart();

## Remarks

None