Jump to main content

##

# 2.106.17 SDMMCx_ModuleInit Function

## C

    /* x = SDMMC instance number */

    void SDMMCx_ModuleInit ( void )

## Summary

Initializes the SDMMC peripheral.

## Description

This function initializes the SDMMC peripheral. The SDMMC peripheral is initialized in 1 bit mode and the SDMMC clock is set to 400 kHz. This function may be called at run time to re-initialize the peripheral to the initial state.

## Precondition

None.

## Parameters

None.

## Returns

None.

## Example

    SDMMC1_ModuleInit();

## Remarks

None.