Jump to main content

##

# 2.99.7 RTC_InterruptDisable Function

## C

    void RTC_InterruptDisable(RTC_INT_MASK interrupt)

## Summary

Disables the specified RTC interrupt

## Description

This function is used to disable a specific RTC interrupt source

## Precondition

None.

## Parameters

Param | Description
--- | ---
interrupt | Interrupt source to be disabled

## Returns

None.

## Example

    RTC_InterruptDisable(RTC_INT_ALARM);