Jump to main content

##

# 1.1.1.5 mtch2120_getDeviceInformation

    MTCH2120_I2C_Status mtch2120_getDeviceInformation(mtch2120_DeviceInformation_t *deviceInformation_l);

## Description:

This function reads device information from the MTCH2120 device via the I2C peripheral.

## Parameter:

Field | Type | Description
--- | --- | ---
deviceInformation_l | mtch2120_DeviceInformation_t* | Device Information structure pointer is required to store the read value.

## Return:

MTCH2120_I2C_Status