Jump to main content

##

# 1.1.1.4 mtch2120_writeToMemory

    MTCH2120_I2C_Status mtch2120_writeToMemory(uint16_t memoryAddress, const uint8_t *data, uint8_t length);

## Description:

This function writes data to the MTCH2120 device memory via the I2C peripheral, according to the specified length.

## Parameters:

Field | Type | Description
--- | --- | ---
memoryAddress | uint16_t | Address of the memory location
data | const uint8_t * | Data that needs to be written.
length | uint8_t | Number of bytes to write

## Return:

MTCH2120_I2C_Status