Jump to main content

# 1.1.3.4.45 DRV_RF215_PLIB_SPI_SET_CS Typedef

## C

    typedef void ( *DRV_RF215_PLIB_SPI_SET_CS ) (SPI_CHIP_SELECT chipSelect);

## Summary

Pointer to a PLIB function to set the SPI chip select line.

## Description

This data type defines the required function signature for the RF215 driver to set the SPI chip select line.

## Parameters

Param | Description
--- | ---
chipSelect | Chip select line to be set.

## Returns

None.

## Remarks

This data type is only available if the used SPI peripheral supports multiple chip select lines.

Rev: G