Jump to main content

# 2.1.10 Build and Program

The demo project will be compiled and programmed to both PIC32CXMTG-EK boards.

1. Build the application.
   1. Open the project Properties by right clicking on the project name (pic32cxmtg).
   2. Ensure that XC32 compiler toolchain is selected. Press OK.
      Figure 2-29.Select Compiler
2. Build the application by clicking on the Build Main Project or Clean and Build Main Project menu command.
   Figure 2-30.Build Project
3. Verify the build is SUCCESSFUL in Output window.
   Figure 2-31.Successful Build
4. Program the application.
   1. Connect a micro-USB cable from computer to the USB port on the PIC32CXMTG-EK board.
   2. Click on Make and Program Device Main Project menu command.
      Figure 2-32.Make And Program Device
5. If not already done, select the programming tool for the connected board.
   Figure 2-33.Select Programming Tool
6. Repeat steps 4 and 5 for the second PIC32CXMTG-EK board.

Rev: G