Jump to main content

# DRV_PLC_PHY_CSMA Struct

## C

    typedef struct {
      /* Use CSMA (0) or forced transmission (1) */
      uint8_t disableRx : 1;
      /* Number of CSMA senses */
      uint8_t senseCount : 3;
      /* CSMA Sense delay in milliseconds */
      uint8_t senseDelayMs : 4;
    } DRV_PLC_PHY_CSMA;

## Summary

Contains the CSMA algorithm related information.

## Description

This data type includes the CSMA algorithm related information. It is used in transmission request object.

## Remarks

None.

Rev: G