Jump to main content

# DRV_PLC_PHY_TRANSMISSION_CFM_OBJ Struct

## G3 DRV_PLC_PHY_TRANSMISSION_CFM_OBJ Struct

### C

    typedef struct {
          /* Instant when frame transmission ended referred to 1us PHY counter */
          uint32_t time;
          /* RMS_CALC it allows to estimate tx power injected */
          uint32_t rmsCalc;
          /* Tx Result (see "TX Result values" above) */
          DRV_PLC_PHY_TX_RESULT result;
    } DRV_PLC_PHY_TRANSMISSION_CFM_OBJ;

### Summary

G3-PLC result of a transmission.

### Description

This data type contains the information of the last transmission, its result, timestamp and an estimation of the injected power.

### Remarks

None.

## PRIME DRV_PLC_PHY_TRANSMISSION_CFM_OBJ Struct

### C

    typedef struct {
        /* Instant when frame transmission started referred to 1us PHY counter */
        uint32_t time;
        /* RMS value emitted */
        uint32_t rmsCalc;
        /* PRIME Frame type */
        DRV_PLC_PHY_FRAME_TYPE frameType;
        /* Tx Result (see "TX Result values" above) */
        DRV_PLC_PHY_TX_RESULT result;
        /* Buffer Id used for transmission */
        DRV_PLC_PHY_BUFFER_ID bufferId;
    } DRV_PLC_PHY_TRANSMISSION_CFM_OBJ;

### Summary

PRIME result of a transmission.

### Description

This structure contains the information of the last transmission, its result, timestamp, an estimation of the injected power and the buffer ID used for transmitting.

### Remarks

None.

## Meters And More DRV_PLC_PHY_TRANSMISSION_CFM_OBJ Struct

### C

    typedef struct {
          /* Instant when frame transmission ended referred to 1us PHY counter */
          uint32_t timeEnd;
          /* RMS_CALC it allows to estimate tx power injected */
          uint32_t rmsCalc;
          /* Tx Result (see "TX Result values" above) */
          DRV_PLC_PHY_TX_RESULT result;
    } DRV_PLC_PHY_TRANSMISSION_CFM_OBJ;

### Summary

Result of a transmission and related parameters.

### Description

This data type contains the information of the last transmission, its result, timestamp and an estimation of the injected power. For result values, see Meters and More DRV_PLC_PHY_TX_RESULT.

### Remarks

None.

Rev: G