Jump to main content

# 2.2.6 Pin Configuration

1. Start Pin Configuration from Plugins drop-down menu.
   Figure 2-54.Start Pin Configuration
2. All pins shown in below figures are automatically configured by the PIC32CXMTSH-DB MCC Component when enabling functionalities or connecting boards to external connectors.
   Figure 2-55.Pin Configuration (1)
   Figure 2-56.Pin Configuration (2)
   Figure 2-57.Pin Configuration (3)
   This configuration follows the Xplained-PRO interface definition for PIC32CXMTSH-DB board used on this example.
   Figure 2-58.PIC32CXMTSH-DB Xplained-PRO

Rev: G