Jump to main content

# DRV_PLC_PHY_SCH Enum

## C

    typedef enum {
        SCHEME_DBPSK = 0,
        SCHEME_DQPSK = 1,
        SCHEME_D8PSK = 2,
        SCHEME_DBPSK_C = 4,
        SCHEME_DQPSK_C = 5,
        SCHEME_D8PSK_C = 6,
        SCHEME_R_DBPSK = 12,
        SCHEME_R_DQPSK = 13,
    } DRV_PLC_PHY_SCH;

## Summary

PRIME Modulation schemes.

## Description

This Enum contains every types of modulation schemes supported by PRIME spec.

Rev: G