Jump to main content

# 1.2.2.4.9 SRV_PSNIFFER_COMMAND Enum

## C - PRIME Implementation

    typedef enum
    {
      /* Set PLC Channel */
      SRV_PSNIFFER_CMD_SET_PLC_CHANNEL = 2,
      /* Set RF Band, Operating Mode and Channel */
      SRV_PSNIFFER_CMD_SET_RF_BAND_OPM_CHANNEL
    } SRV_PSNIFFER_COMMAND;

## C - G3 Implementation

    dtypedef enum
    {
      /* Receive new message */
      SRV_PSNIFFER_CMD_RECEIVE_MSG = 0,
      /* Set PLC Tone Mask */
      SRV_PSNIFFER_CMD_SET_PLC_TONE_MASK,
      /* Set RF Band, Operating Mode and Channel */
      SRV_PSNIFFER_CMD_SET_RF_BAND_OPM_CHANNEL
    } SRV_PSNIFFER_COMMAND;

## Summary

Hybrid Sniffer Tool Commands enumeration.

## Description

This enumeration defines the commands used by the Hybrid PHY Sniffer tool provided by Microchip.

Rev: G