Jump to main content

# 1.2.1.4.2 Library Interface (PRIME)

If the PLC Driver uses PRIME PHY, the PLC PHY Coupling service library provides the following interfaces:

Functions

Name | Description
--- | ---
SRV_PCOUP_Get_Default_Channel | Get the default PRIME channel
SRV_PCOUP_Get_Channel_Config | Get the PLC PHY Coupling parameters for the specified PRIME channel
SRV_PCOUP_Set_Channel_Config | Set the PLC PHY Coupling parameters for the specified PRIME channel

Data types and constants

Name | Type | Description
--- | --- | ---
SRV_PLC_PCOUP_CHANNEL_DATA | Struct | PLC PHY Coupling data

Rev: G