Jump to main content

# 1.1.2.4.64 MAC_RT_TONE_MAP_RESPONSE Struct

## C

    typedef struct {
        MAC_RT_MOD_SCHEME modScheme;
        MAC_RT_MOD_TYPE modType;
        uint8_t txGain;
        uint8_t txRes;
        MAC_RT_TONE_MAP toneMap;
        uint8_t reserved1;
        uint8_t lqi;
        MAC_RT_TX_COEF txCoef;
        uint8_t reserved2;
    } MAC_RT_TONE_MAP_RESPONSE;

## Summary

G3-PLC MAC Tone Map Response.

## Description

This data type includes information related to the G3-PLC Tone Map Response frame.

## Remarks

For additional information, refer to the G3-PLC Specification.

Rev: G