Jump to main content

# 1.1.3.4.3 DRV_RF215_Tasks Function

## C

    void DRV_RF215_Tasks( SYS_MODULE_OBJ object );

## Summary

Maintains the RF215 driver's state machine.

## Description

This function is used to maintain the RF215 driver's internal state machine.

## Precondition

The DRV_RF215_Initialize routine must have been called to obtain a valid system object.

## Parameters

Param | Description
--- | ---
object | Driver object handle, returned from the DRV_RF215_Initialize routine.

## Returns

None.

## Example

    SYS_MODULE_OBJ sysObjDrvRf215; // Returned from DRV_RF215_Initialize

    while (true)
    {
        DRV_RF215_Tasks (sysObjDrvRf215);

        // Do other tasks
    }

## Remarks

This function is normally not called directly by an application. It is called by the system's tasks routine (SYS_Tasks).

Rev: G