Jump to main content

# 1.1.3.4.42 DRV_RF215_TX_CONFIRM_OBJ Struct

## C

    typedef struct
    {
        /* TX time (PPDU start), referred to system 64-bit time counter */
        uint64_t                     timeIniCount;

        /* PPDU duration in system time counter units */
        uint32_t                     ppduDurationCount;

        /* Transmission result */
        DRV_RF215_TX_RESULT          txResult;

    } DRV_RF215_TX_CONFIRM_OBJ;

## Summary

Defines the data reported in RF215 TX confirm.

## Description

This data type defines the data reported in the RF215 transmit confirm callback function (DRV_RF215_RX_IND_CALLBACK).

## Remarks

The `timeIni` parameter is only available if PHY TX/RX time support is enabled through MCC.

Rev: G