Jump to main content

# 1.1.3.4.32 DRV_RF215_TX_TIME_MODE Enum

## C

    typedef enum
    {
        /* Absolute time, referred to system 64-bit counter */
        TX_TIME_ABSOLUTE = 0,

        /* Relative time, referred to current system time */
        TX_TIME_RELATIVE = 1,

    } DRV_RF215_TX_TIME_MODE;

## Summary

Defines the available TX time modes.

## Description

This data type defines the list of available Transmission time modes. It is used as parameter in TX request.

## Remarks

None.

Rev: G