Jump to main content

# 1.1.4.61 DRV_METROLOGY_SYN_DESCRIPTOR Struct

## C

    typedef struct {
        DRV_METROLOGY_SYN_CONTROL control;
        uint32_t *pData;
        struct DRV_METROLOGY_SYN_DESCRIPTOR *next;
        struct DRV_METROLOGY_SYN_DESCRIPTOR *prev;
    } DRV_METROLOGY_SYN_DESCRIPTOR;

## Summary

Data descriptor used to configure the synthesizer function.

## Description

Field description:

- control: Synthesizer control values. See DRV_METROLOGY_SYNTHESIZER_CONTROL.
- *pData: Pointer to the data buffer with the waveform samples
- *next: Pointer to the next descriptor address. If NULL, the descriptor is the last one to be performed.
- *prev: Pointer to the previous descriptor address. If NULL, the descriptor is the first one to be performed.

Rev: E