Jump to main content

# 2.1.4.43 DRV_MCMETROLOGY_AFE_DATA Struct

## C

    typedefstruct {
        DRV_MCMETROLOGY_AFE_EVENTS events;
        float chnMeasure[DRV_MCMETROLOGY_CHANNELS_NUMBER][CHN_MEASURE_TYPE_NUM];
        float powMeasure[DRV_MCMETROLOGY_POWERS_NUMBER][POW_MEASURE_TYPE_NUM];
        float measure[MEASURE_TYPE_NUM];
    } DRV_MCMETROLOGY_AFE_DATA;

## Summary

Identifies the data calculated from the Metrology AFE measurements.

## Description

Field description:

- events: AFE events data
- chnMeasure: Measure calculated values depending on channel
- powMeasure: Measure calculated values depending on power source
- measure: Generic Measures calculated values

## Remarks

None.

Rev: E