Jump to main content

# 3.3.4.4 EMAFE_SetSincDecimationFiltersReset Function

## C

    void EMAFE_SetSincDecimationFiltersReset ( bool enable );

## Summary

Enters/exits the reset state of low-pass filters.

## Description

Enters/exits the reset state of low-pass filters.

## Precondition

None.

## Parameters

Parameters | Description
--- | ---
enable | If True, the sinc decimation low-pass filters are in reset state. False, it exits the reset state of low-pass filters.

## Returns

None.

## Example

    /* Decimation LPFIF Filters exits the reset state */
    EMAFE_SetSincDecimationFiltersReset(false);

## Remarks

None.

Rev: E