Jump to main content

# 2.1.4.40 DRV_MCMETROLOGY_HARMONICS_RMS Struct

## C

    typedefstruct {
        double CHx_m_RMS[DRV_MCMETROLOGY_CHANNELS_NUMBER];
    } DRV_MCMETROLOGY_HARMONICS_RMS;

## Summary

Identifies the result of the harmonic analysis process.

## Description

Field description:

- CHx_m_RMS: RMS current value obtained as the result of last the harmonic analysis regarding channel X

## Remarks

None.

Rev: E