Jump to main content

# 1.1.4.36 DRV_METROLOGY_CaptureGetState Function

## C

    uint32_t DRV_METROLOGY_CaptureGetOffset(void);

## Summary

Get the offset of the capture process.

## Description

Offset within the buffer indicating the position of the last sample stored.

## Parameters

None.

## Returns

Capture offset.

## Example

        uint32_t offset;

        offset = DRV_METROLOGY_CaptureGetOffset();

## Remarks

None.

Rev: E