Jump to main content

# 1.1.4.12 DRV_METROLOGY_HARMONICS_CALLBACK Typedef

## C

    typedefvoid (* DRV_METROLOGY_HARMONICS_CALLBACK)(uint32_t harmonicBitmap);

## Summary

Defines the data type and function signature for the callback function of the Harmonics analysis.

## Description

The Metrology driver will call back the client's function with this signature when the Harmonics analysis has been completed.

## Parameters

Parameters | Description
--- | ---
harmonicBitmap | Bitmap defining analyzed harmonics. Each bit set represents one harmonic.

## Returns

None.

## Remarks

None.

Rev: E