Jump to main content

# 1.1.4.41 DRV_METROLOGY_AFE_TYPE Enum

## C

    typedef enum {
        AFE_1xATSENSE203 = 0,
        AFE_1xATSENSE301 = 0,
        AFE_3xMCP1910  = 1,
        AFE_4xMCP1910  = 2,
        AFE_1xMCP3912  = 3,
        AFE_1xMCP3913  = 4,
        AFE_1xMCP3914  = 5,
        AFE_NUM_TYPE
    } DRV_METROLOGY_AFE_TYPE;

## Summary

Describes the AFE type.

## Description

Different AFEs can be used by the Metrology solution, this type enumerates the supported combinations.

Note: AFE_1xATSENSE203 applies to PIC32CXMTSH device (AFE is stacked), while the other combinations can be connected to PIC32CXMTC device.

Rev: E