Jump to main content

# 3.3.4.53 EMAFE_ADCIsAnalogSystemReady Function

## C

    void EMAFE_ADCIsAnalogSystemReady(void);

## Summary

Check if Analog System is ready.

## Description

Check if Analog System is ready.

## Precondition

None.

## Parameters

None.

## Returns

True if Analog System is ready.

## Example

    if (EMAFE_ADCIsAnalogSystemReady())
    {
            // Analog System is ready
    }

## Remarks

Each time a software or hardware reset is performed, the analog is initialized. Analog System is true indicates the end of initialization periods.

Important: When Analog System is false, configuration must not be performed.

Rev: E