Jump to main content

# 3.3.4.52 EMAFE_ADCIsLDOEnable Function

## C

    void EMAFE_ADCIsLDOEnable(void);

## Summary

Check if Internal LDO is enabled.

## Description

Check if Internal LDO is enabled.

## Precondition

None.

## Parameters

None.

## Returns

True if Internal LDO is enabled.

## Example

    if (EMAFE_ADCIsLDOEnable())
    {
            // Internal LDO is enabled
    }

## Remarks

Note: When LDO is written to 1, it can be read at one after 768 μs.

Rev: E