Jump to main content

# 1.1.4.10 DRV_METROLOGY_CALIBRATION_CALLBACK Typedef

## C

    typedef void (* DRV_METROLOGY_CALIBRATION_CALLBACK)(bool result);

## Summary

Defines the data type and function signature for the callback function of the calibration procedure.

## Description

The Metrology driver will call back the client's function with this signature when the Calibration procedure has been completed.

## Parameters

Parameters | Description
--- | ---
result | Flag o indicate if at least one channel has been calibrated successfully. Otherwise none of the channels have been calibrated.

## Returns

None.

## Remarks

None.

Rev: E