Jump to main content

# 3.3.4.24 EMAFE_GetStatus Function

## C

    uint32_t EMAFE_GetStatus(void);

## Summary

Read comparison events on Channel A and B.

## Description

Read comparison events on Channel A and B.

## Precondition

None.

## Parameters

None.

## Returns

Events status.

## Example

    evantsStatus = EMAFE_GetStatus();

## Remarks

Table 3-16.Status Description
Status Mask | Description When Value = 1
--- | ---
EMAFE_SR_CHAEVT_Msk | Comparison event on Channel A; Channel A is not in the range
EMAFE_SR_CHBEVT_Msk | Comparison event on Channel B; Channel B is not in the range

Rev: E