Jump to main content

# 2.1.4.10 DRV_MCMETROLOGY_HARMONICS_CALLBACK Typedef

## C

    typedefvoid (* DRV_MCMETROLOGY_HARMONICS_CALLBACK)(uint8_t harmonicNum);

## Summary

Defines the data type and function signature for the callback function of the Harmonics analysis.

## Description

The Metrology driver will call back the client's function with this signature when the Harmonics analysis has been completed.

## Parameters

Parameters | Description
--- | ---
harmonicNum | The number of the harmonic that has been analyzed

## Returns

None.

## Remarks

None.

Rev: E