Jump to main content

# 1.1.4.60 DRV_METROLOGY_SYN_CONTROL Struct

## C

    typedef struct {
        unsigned int numSamples : 19;
        unsigned int channel : 5;
        unsigned int key : 8;
    } DRV_METROLOGY_SYN_CONTROL;

## Summary

Control fields for the synthesizer function.

## Description

Field description:

- numSamples: Number of samples to be transferred
- channel: Indicates the channel number to which the samples belong to
- key: Security key. It must be set to DRV_METROLOGY_SYNTHESIZER_CONTROL_KEY.

Rev: E