Jump to main content

# 1.1.4.13 DRV_METROLOGY_GetAFEDescription Function

## C

    DRV_METROLOGY_AFE_TYPE DRV_METROLOGY_GetAFEDescription (char *pDescription);

## Summary

Get the AFE type.

## Description

AFE type returned by this function provides information about the ATSENSE/MCP(s) device(s) connected to metrology library.

## Parameters

Parameters | Description
--- | ---
pDescription | Pointer to string where description will be written

## Returns

AFE type. For available types see DRV_METROLOGY_AFE_TYPE Enum.

## Example

    char afeDesc[30];

    app_metrologyData.afe = DRV_METROLOGY_GetAFEDescription(afeDesc);

## Remarks

None.

Rev: E