Jump to main content

##

# TCPIP_IPV6_Put Function

## C

    bool TCPIP_IPV6_Put(
        IPV6_PACKET * pkt,
        unsigned char v
    );

## Description

This function writes a character of data to a packet.

## Preconditions

TCPIP_IPV6_Initialize() is required. TCPIP_IPV6_InterfaceIsReady should be true.

## Parameters

Parameters | Description
--- | ---
pkt | The packet.
v | The character.

## Returns

- True - If the character was written.
- False - If the character was not written.

## Remarks

None.