Jump to main content

##

# TCPIP_IPV6_IsFragmentationEnabled Function

## C

    TCPIP_IPV6_IsFragmentationEnabled();

## Description

This function is a helper to return the IPv6 fragmentation support.

## Preconditions

IPv6 properly initialized.

## Returns

- True - If the fragmentation is enabled and supported by the IPv6 module.
- False - Fragmentation is not supported.

## Remarks

The IPv6 fragmentation support is always enabled.