Jump to main content

##

# NET_PRES_Status Function

## C

    SYS_STATUS NET_PRES_Status(SYS_MODULE_OBJ object);

## Returns

- SYS_STATUS_READY - Indicates that any previous module operation for the specified module has completed

- SYS_STATUS_UNINITIALIZED - Indicates the module has not been initialized

- SYS_STATUS_BUSY - Indicates that the module is busy and can't accept operations

- SYS_STATUS_ERROR - Indicates that there is a fatal error in the module

## Description

This function provides the current status of the MPLAB Harmony Net Presentation Layer.

## Remarks

None.

## Preconditions

The NET_PRES_Initialize function must have been called before calling this function. Networking Presentation Layer Help Library Interface b) Socket Functions

## Parameters

Parameters | Description
--- | ---
object | Layer object handle, returned from NET_PRES_Initialize