Jump to main content

##

# DRV_ETHPHY_NEGOTIATION_RESULT Structure

## C

    typedef struct {
        DRV_ETHPHY_LINK_STATUS linkStatus;
        TCPIP_ETH_OPEN_FLAGS linkFlags;
        TCPIP_ETH_PAUSE_TYPE pauseType;
    } DRV_ETHPHY_NEGOTIATION_RESULT;

## Members

Members | Description
--- | ---
DRV_ETHPHY_LINK_STATUS linkStatus; | link status after a completed negotiation
TCPIP_ETH_OPEN_FLAGS linkFlags; | the negotiation result flags
TCPIP_ETH_PAUSE_TYPE pauseType; | pause type supported by the link partner

## Description

Ethernet PHY Device Driver Negotiation result Data Contains all the data necessary to get the Ethernet PHY negotiation result

## Remarks

A pointer to a structure of this format must be passed into the DRV_ETHPHY_NegotiationResultGet routine.