Jump to main content

##

# TCPIP_TCP_FifoTxFullGet Function

## C

    uint16_t TCPIP_TCP_FifoTxFullGet(
        TCP_SOCKET hTCP
    );

## Description

This function determines how many bytes are pending in the TCP TX FIFO.

## Preconditions

TCP is initialized.

## Parameters

Parameters | Description
--- | ---
hTCP | The socket to check.

## Returns

Number of bytes pending to be flushed in the TCP TX FIFO.

## Remarks

None.