Jump to main content

##

# DRV_MIIM_SETUP Structure

## C

    C
    typedef struct {
        uint32_t hostClockFreq;
        uint32_t maxBusFreq;
        DRV_MIIM_SETUP_FLAGS setupFlags;
    } DRV_MIIM_SETUP;

## Members

Members | Description
--- | ---
uint32_t hostClockFreq; | The clock frequency on which this MIIM module operates on, Hz
uint32_t maxBusFreq; | The MIIM bus maximum supported frequency, Hz This is a maximum value. The actual generated value may differ.
DRV_MIIM_SETUP_FLAGS setupFlags; | Setup flags

## Description

MIIM Device Driver Set up Data This data structure contains all the data necessary to configure the MIIM device.

## Remarks

A pointer to a structure of this format containing the desired initialization data must be passed into the DRV_MIIM_Setup routine.