Jump to main content

##

# TCPIP_ANNOUNCE_BROADCAST_TYPE Enumeration

## C

    typedef enum {
        TCPIP_ANNOUNCE_BCAST_NONE,
        TCPIP_ANNOUNCE_BCAST_NET_LIMITED,
        TCPIP_ANNOUNCE_BCAST_NET_DIRECTED
    } TCPIP_ANNOUNCE_BROADCAST_TYPE;

## Description

Enumeration: TCPIP_ANNOUNCE_BROADCAST_TYPE - Describes the current message types supported by the announce module.

## Members

Members | Description
--- | ---
TCPIP_ANNOUNCE_BCAST_NONE | invalid, not specified.
TCPIP_ANNOUNCE_BCAST_NET_LIMITED | the Announce messages will be sent using the IPv4 network limited broadcast type, i.e 255.255.255.255. This is the default.
TCPIP_ANNOUNCE_BCAST_NET_DIRECTED | the Announce messages will be sent using the IPv4 network directed broadcast type, i.e 192.168.1.255 for example.