Jump to main content

##

# TCPIP_STACK_NetAddressBcast Function

## C

    uint32_t TCPIP_STACK_NetAddressBcast(
        TCPIP_NET_HANDLE netH
    );

## Description

The function returns the network interface broadcast address. The interface should be enabled for this function to work.

## Preconditions

The TCPIP_STACK_Initialize() function must have been called before calling this function. The network interface should be up and running.

## Parameters

Parameters | Description
--- | ---
netH | Interface handle to get address of.

## Returns

- Broadcast IP address of that interface.
- 0 if no such interface.

## Remarks

None.