Jump to main content

##

# TCPIP_DHCPS_MODULE_CONFIG Structure

## C

    typedef struct {
    bool enabled;
    bool deleteOldLease;
    size_t leaseEntries;
    uint32_t entrySolvedTmo;
    TCPIP_DHCPS_ADDRESS_CONFIG * dhcpServer;
    } TCPIP_DHCPS_MODULE_CONFIG;

## Description

Structure: TCPIP_DHCPS_MODULE_CONFIG.

DHCP server configuration and initialization data . Configuration is part of tcpip_stack_init.c.

## Members

Members | Description
--- | ---
enabled | Enable DHCP server.
deleteOldLease | Delete old cache if still in place, specific DHCP parameters.
leaseEntries | Max number of lease entries.
entrySolvedTmo | Solved entry removed after this tmo in seconds.
dhcpServer | DHCP server lease address configuration details uint32_t dhcpServerCnt; // Max DHCP server support.