Jump to main content

##

# TCPIP_IPV6_MulticastListenerAdd Function

## C

    IPV6_ADDR_STRUCT * TCPIP_IPV6_MulticastListenerAdd(
        TCPIP_NET_HANDLE hNet,
        IPV6_ADDR * address
    );

## Description

This function is used to add the IPv6 multicast address to an interface.

## Preconditions

TCPIP_IPV6_Initialize() should be called. TCPIP_IPV6_InterfaceIsReady should be true.

## Parameters

Parameters | Description
--- | ---
netH | The interface to add the address.
address | The address.

## Returns

IPV6_ADDR_STRUCT *

- On Success - Pointer to the new listener.
- On Failure - NULL.

## Remarks

None.