Jump to main content

##

# DRV_MIIM_ClientStatus Function

## C

    DRV_MIIM_CLIENT_STATUS DRV_MIIM_ClientStatus(DRV_HANDLE handle);

## Returns

- DRV_MIIM_CLIENT_STATUS_READY - if the client handle represents a valid MIIM client

- DRV_MIIM_CLIENT_STATUS_ERROR - if the client handle is an invalid MIIM client

## Description

This function gets the client-specific status of the MIIM driver associated with the given handle.

## Remarks

This function can be used to check that a client handle points to a valid MIIM client. The MIIM driver queues operations so it will always return DRV_MIIM_CLIENT_STATUS_READY.

## Preconditions

- The DRV_MIIM_Initialize routine must have been called.

- DRV_MIIM_Open must have been called to obtain a valid opened device handle.