Jump to main content

##

# DRV_ENC28J60_Close Function

## C

    void DRV_ENC28J60_Close(DRV_HANDLE handle);

## Returns

None.

## Description

ENC28J60 Close This function closes a handle to the driver. If it is the last client open, the driver will send an RX Disable command to the ENC hardware and move to the closed state.

## Preconditions

The client had to be successfully opened with DRV_ENC28J60_Open.

## Parameters

Parameters | Description
--- | ---
handle | The successfully opened handle