Jump to main content

##

# TCPIP_SMTPC_ATTACH_TYPE Enumeration

## C

    typedef enum {
        TCPIP_SMTPC_ATTACH_TYPE_UNKNOWN = 0x0000,
        TCPIP_SMTPC_ATTACH_TYPE_APPLICATION = 0x0001,
        TCPIP_SMTPC_ATTACH_TYPE_TEXT = 0x0002,
        TCPIP_SMTPC_ATTACH_TYPE_INLINE = 0x8000
    } TCPIP_SMTPC_ATTACH_TYPE;

## Description

Enumeration: TCPIP_SMTPC_ATTACH_TYPE.

Enumeration describing the possible attachment types supported by the SMTPC client.

## Members

Members | Description
--- | ---
TCPIP_SMTPC_ATTACH_TYPE_UNKNOWN = 0x0000 | Unknown attachment type; will default to binary.
TCPIP_SMTPC_ATTACH_TYPE_APPLICATION = 0x0001 | Application octet stream, binary Use this attachment type when sending binary data.
TCPIP_SMTPC_ATTACH_TYPE_TEXT = 0x0002 | Plain text. Use this attachment type when sending ASCII text. Other supported types will be added here.
TCPIP_SMTPC_ATTACH_TYPE_INLINE = 0x8000 | Flag for sending the data as inline instead of attachment.

## Remarks

Only one attachment type should be set at a time.