Jump to main content

##

# DRV_MIIM_OPERATION_FLAGS Enumeration

## C

    typedef enum {
        DRV_MIIM_OPERATION_FLAG_NONE,
        DRV_MIIM_OPERATION_FLAG_DISCARD
    } DRV_MIIM_OPERATION_FLAGS;

## Members

Members | Description
--- | ---
DRV_MIIM_OPERATION_FLAG_NONE | No flag specified
DRV_MIIM_OPERATION_FLAG_DISCARD | Upon completion discard the operation result. The client will not poll to check the result nor will need notification This allows dummy operations, discarded as they complete

## Description

MIIM Driver Operation flags This enumeration identifies the operation-specific flags supported by the MIIM driver.

## Remarks

Currently only 8 bit flags are supported. Multiple flags can be simultaneously set.