Jump to main content

##

# DRV_ENCX24J600_LinkCheck Function

## C

    bool DRV_ENCX24J600_LinkCheck(DRV_HANDLE hMac);

## Returns

- true - if the link is active
- false - all other times

## Description

ENCX24J600 Link Check This function checks the status of the link and returns it to the caller.

## Preconditions

The client had to be successfully opened with DRV_ENCX24J600_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle