Jump to main content

##

# DRV_ETHPHY_INTERFACE_INDEX Enumeration

## C

    typedef enum {
        DRV_ETHPHY_INF_IDX_ALL_EXTERNAL,
        DRV_ETHPHY_INF_IDX_PORT_0,
        DRV_ETHPHY_INF_IDX_PORT_1,
        DRV_ETHPHY_INF_IDX_PORT_2,
        DRV_ETHPHY_INF_IDX_PORT_3,
        DRV_ETHPHY_INF_IDX_PORT_4,
        DRV_ETHPHY_INF_IDX_PORT_5
    } DRV_ETHPHY_INTERFACE_INDEX;

## Members

Members | Description
--- | ---
DRV_ETHPHY_INF_IDX_ALL_EXTERNAL | All External Interfaces
DRV_ETHPHY_INF_IDX_PORT_0 | Port 0 interface
DRV_ETHPHY_INF_IDX_PORT_1 | Port 1 interface
DRV_ETHPHY_INF_IDX_PORT_2 | Port 2 interface
DRV_ETHPHY_INF_IDX_PORT_3 | Port 3 interface
DRV_ETHPHY_INF_IDX_PORT_4 | Port 4 interface
DRV_ETHPHY_INF_IDX_PORT_5 | Port 5 interface

## Description

Ethernet PHY Interface Index This enumeration defines the index type supported by the PHY Used by: DRV_ETHPHY_PhyAddressGet, DRV_ETHPHY_RestartNegotiation, DRV_ETHPHY_NegotiationIsComplete, DRV_ETHPHY_LinkStatusGet