Jump to main content

##

# TCPIP_DNS_CLIENT_MAX_SELECT_INTERFACES Macro

## C

    #define TCPIP_DNS_CLIENT_MAX_SELECT_INTERFACES 4

## Description

Max number of interfaces to take part in the DNS selection algorithm Should be always greater than 1:

- the default interface should always be considered for DNS resolution

Depending on how many active interfaces select those to be considered for DNS resolution.