Jump to main content

##

# DRV_ENCX24J600_Process Function

## C

    TCPIP_MAC_RES DRV_ENCX24J600_Process(DRV_HANDLE hMac);

## Returns

- TCPIP_MAC_RES_TYPE_ERR - if the hMac is invalid
- TCPIP_MAC_RES_OP_ERR - if the hMac is valid

## Description

ENCX24J600 Process This function does additional processing that is not done inside the tasks function.

## Remarks

This function does nothing in the first release.

## Preconditions

The client had to be successfully opened with DRV_ENCX24J600_Open.

## Parameters

Parameters | Description
--- | ---
hMac | the successfully opened handle